Dummy gx.dll
                    Ver 0.4  2004/07/20
                    by k-matsu ( http://www.age.jp/~k-matsu/ )

GAPI improves Video playback dramatically.

Most new ARM devices can use the excellent GAPI implementation made by WinCE Soft 
(http://www.wincesoft.de/html/gapi_for_hpc_s.html).

However it is quite difficult to find a working GX.dll for MIPS and CE 2.11 devices.

The included version works very well with TCPMP/BetaPlayer. Install it before your HPC Media Player.

Choose the correct device ( OS version and processor type): copy the required gx.dll and the correct gx.dll.ini to your Windows folder.

You can find different gx.dll.ini templates for many devices in this package: rename the "some_device.gx.dll.ini" to "gx.dll.ini".
If you don't find your device, you may have to manually edit some gx.dll.ini ( check the screen size).


